# -*- text -*-
# Copyright (C) 2015 The FreeRADIUS Server project and contributors
#
#	Attributes and values defined in RFC 4675.
#	http://www.ietf.org/rfc/rfc4675.txt
#
#	$Id: d615722b7d763b344558eac17b12a6a607014b0e $
#

#
#  High byte = '1' (0x31) means the frames are tagged.
#  High byte = '2' (0x32) means the frames are untagged.
#
#  Next 12 bits MUST be zero.
#
#  Lower 12 bits is the IEEE-802.1Q VLAN VID.
#
ATTRIBUTE	Egress-VLANID				56	integer
ATTRIBUTE	Ingress-Filters				57	integer

#
#  First byte == '1' (0x31) means that the frames are tagged.
#  First byte == '2' (0x32) means that the frames are untagged.
#
ATTRIBUTE	Egress-VLAN-Name			58	string
ATTRIBUTE	User-Priority-Table			59	octets # 8

VALUE	Ingress-Filters			Enabled			1
VALUE	Ingress-Filters			Disabled		2
