# -*- text -*-
# Copyright (C) 2015 The FreeRADIUS Server project and contributors
#
#        Attributes and values defined in RFC 7268
#        http://www.ietf.org/rfc/rfc7268.txt
#
#	$Id: e01186a235cde7d51fe1e271c5096da01faa5f2e $
#

ATTRIBUTE	Allowed-Called-Station-Id		174	string
ATTRIBUTE	EAP-Peer-Id				175	octets
ATTRIBUTE	EAP-Server-Id				176	octets
ATTRIBUTE	Mobility-Domain-Id			177	integer
ATTRIBUTE	Preauth-Timeout				178	integer
ATTRIBUTE	Network-Id-Name				179	octets

# TLVs in the format defined in Figure 11-8 of Section 11.12 of
# "IEEE Standard for Local and metropolitan area
# networks - Port-Based Network Access Control", IEEE Std
# 802.1X-2010.
#
# These are <drum roll> 7 bit TLV-Type, and 9-bit TLV-Length
#
# If the TLVs are too large for 253 octets, they are fragmented
# into multiple attributes.
ATTRIBUTE	EAPoL-Announcement			180	octets	concat

ATTRIBUTE	WLAN-HESSID				181	string

# The upper two octets MUST be zero.
# low two octets are Venue-Group and Venue-Type.
# Defined in Section 8.4.1.34 of the above IEEE document.
ATTRIBUTE	WLAN-Venue-Info				182	integer

# A two or 3 character language code selected from ISO-639.
# If it's two characters, a trailing zero byte is added
ATTRIBUTE	WLAN-Venue-Language			183	octets[3]

ATTRIBUTE	WLAN-Venue-Name				184	string

# two least significant octets contain the Reason Code values defined
# in Table 8-36 of Section 8.4.1.7 of the above IEEE document.
ATTRIBUTE	WLAN-Reason-Code			185	integer

# The next four attributes are binary packed.  The first 3 octets is
# the OUI.  The last octet is the Suite Type.

# in Suite selector format as specified in Figure 8-187 within Section
# 8.4.2.27.2 of [IEEE-802.11], with values of OUI and Suite Type drawn
# from Table 8-99.
ATTRIBUTE	WLAN-Pairwise-Cipher			186	integer

# same as WLAN-Pairwise-Cipher
ATTRIBUTE	WLAN-Group-Cipher			187	integer

# in Suite selector format as specified in Figure 8-187
# within Section 8.4.2.27.2 of [IEEE-802.11], with values of OUI and
# Suite Type drawn from Table 8-101:
ATTRIBUTE	WLAN-AKM-Suite				188	integer

# same as WLAN-Pairwise-Cipher
ATTRIBUTE	WLAN-Group-Mgmt-Cipher			189	integer

# the upper 3 octets are zero
# the low octet contains the RF Band field, whose values are defined
# by the IEEE 802.11 Band ID field (Table 8-53a of [IEEE-802.11ad])

ATTRIBUTE	WLAN-RF-Band				190	integer

