# -*- text -*-
##############################################################################
#
#	Alcatel-Lucent Service Router dictionary.
#
#	$Id$
#
##############################################################################

VENDOR		Alcatel-Lucent-Service-Router	6527

BEGIN-VENDOR	Alcatel-Lucent-Service-Router

# Alcatel Timetra attributes
ATTRIBUTE	Timetra-Access				1	integer
ATTRIBUTE	Timetra-Home-Directory			2	string
ATTRIBUTE	Timetra-Restrict-To-Home		3	integer
ATTRIBUTE	Timetra-Profile				4	string
ATTRIBUTE	Timetra-Default-Action			5	integer
ATTRIBUTE	Timetra-Cmd				6	string
ATTRIBUTE	Timetra-Action				7	integer
ATTRIBUTE	Timetra-Exec-File			8	string

VALUE	Timetra-Access			ftp			1
VALUE	Timetra-Access			console			2
VALUE	Timetra-Access			both			3

VALUE	Timetra-Restrict-To-Home	true			1
VALUE	Timetra-Restrict-To-Home	false			2

VALUE	Timetra-Default-Action		permit-all		1
VALUE	Timetra-Default-Action		deny-all		2
VALUE	Timetra-Default-Action		none			3

VALUE	Timetra-Action			permit			1
VALUE	Timetra-Action			deny			2

# Alcatel Timetra authorization and CoA VSA
ATTRIBUTE	Alc-Primary-Dns				9	ipaddr
ATTRIBUTE	Alc-Secondary-Dns			10	ipaddr
ATTRIBUTE	Alc-Subsc-ID-Str			11	string
ATTRIBUTE	Alc-Subsc-Prof-Str			12	string
ATTRIBUTE	Alc-SLA-Prof-Str			13	string
ATTRIBUTE	Alc-Force-Renew				14	string
ATTRIBUTE	Alc-Create-Host				15	string
ATTRIBUTE	Alc-ANCP-Str				16	string
ATTRIBUTE	Alc-Retail-Serv-Id			17	integer
ATTRIBUTE	Alc-Retail-Serv-Id			17	integer
ATTRIBUTE	Alc-Default-Router			18	ipaddr
ATTRIBUTE	Alc-Client-Hardware-Addr		27	string

# RADIUS subscriber accounting VSAs
ATTRIBUTE	Alc-Acct-I-Inprof-Octets-64		19	integer
ATTRIBUTE	Alc-Acct-I-Outprof-Octets-64		20	integer
ATTRIBUTE	Alc-Acct-O-Inprof-Octets-64		21	integer
ATTRIBUTE	Alc-Acct-O-Outprof-Octets-64		22	integer
ATTRIBUTE	Alc-Acct-I-Inprof-Pkts-64		23	integer
ATTRIBUTE	Alc-Acct-I-Outprof-Pkts-64		24	integer
ATTRIBUTE	Alc-Acct-O-Inprof-Pkts-64		25	integer
ATTRIBUTE	Alc-Acct-O-Outprof-Pkts-64		26	integer

# Used when authenticating migrant hosts
ATTRIBUTE   Alc-Wlan-Portal-Redirect                  172 string

# If a migrant host is redirected, specifies the URL
ATTRIBUTE   Alc-Wlan-Portal-Url                       173 string

# Defines the lease-time in seconds for RADIUS proxy and create-host-CoA
# scenarios only.
ATTRIBUTE   Alc-Lease-Time                            174 integer

# The URL to which traffic matching the host IPv4 filter entry with http-redirect
# action is redirected to
ATTRIBUTE   Alc-Portal-Url                            177 string

# names longer than the allowed maximum are treated as host setup failures
ATTRIBUTE   Alc-SLAAC-IPv6-Pool                       181 string

END-VENDOR	Alcatel-Lucent-Service-Router
