# -*- text -*-
# Copyright (C) 2015 The FreeRADIUS Server project and contributors
#
#	Altiga vendor attributes
#
#	Altiga networks was acquired by Cisco in 2000.
#
#	$Id: 66c75d2dd2b8f5f439a6ddca7513db17b9eeff0d $
#

VENDOR		Altiga				3076

BEGIN-VENDOR	Altiga
ATTRIBUTE	Altiga-Access-Hours-G/U                 1	string
ATTRIBUTE	Altiga-Simultaneous-Logins-G/U          2	integer
ATTRIBUTE	Altiga-Min-Password-Length-G		3	integer
ATTRIBUTE	Altiga-Allow-Alpha-Only-Passwords-G	4	integer
ATTRIBUTE	Altiga-Primary-DNS-G			5	ipaddr
ATTRIBUTE	Altiga-Secondary-DNS-G			6	ipaddr
ATTRIBUTE	Altiga-Primary-WINS-G			7	ipaddr
ATTRIBUTE	Altiga-Secondary-WINS-G			8	ipaddr
ATTRIBUTE	Altiga-SEP-Card-Assignment-G/U          9	integer
ATTRIBUTE	Altiga-Priority-on-SEP-G/U              10	integer
ATTRIBUTE	Altiga-Tunneling-Protocols-G/U          11	integer
ATTRIBUTE	Altiga-IPSec-Sec-Association-G/U        12	string
ATTRIBUTE	Altiga-IPSec-Authentication-G		13	integer
ATTRIBUTE	Altiga-IPSec-Banner-G			15	string
ATTRIBUTE	Altiga-IPSec-Allow-Passwd-Store-G/U     16	integer
ATTRIBUTE	Altiga-Use-Client-Address-G/U           17	integer
ATTRIBUTE	Altiga-PPTP-Min-Authentication-G/U      18	integer
ATTRIBUTE	Altiga-L2TP-Min-Authentication-G/U      19	integer
ATTRIBUTE	Altiga-PPTP-Encryption-G		20	integer
ATTRIBUTE	Altiga-L2TP-Encryption-G		21	integer
ATTRIBUTE	Altiga-Argument-Authentication-Server-Type 22	integer
ATTRIBUTE	Altiga-IPSec-L2L-Keepalives-G		25	integer
ATTRIBUTE	Altiga-Argument-IPSec-Group-Name	26	integer
ATTRIBUTE	Altiga-IPSec-Split-Tunnel-List-G	27	string
ATTRIBUTE	Altiga-IPSec-Default-Domain-G		28	string
ATTRIBUTE	Altiga-IPSec-Secondary-Domains-G	29	string
ATTRIBUTE	Altiga-IPSec-Tunnel-Type-G		30	integer
ATTRIBUTE	Altiga-IPSec-Mode-Config-G		31	integer
ATTRIBUTE	Altiga-Argument-Authentication-Server-Priority 32	integer
ATTRIBUTE	Altiga-IPSec-User-Group-Lock-G		33	integer
ATTRIBUTE	Altiga-IPSec-Over-NAT-G			34	integer
ATTRIBUTE	Altiga-IPSec-Over-NAT-Port-Num-G	35	integer
ATTRIBUTE	Altiga-Partitioning-Primary-DHCP	128	ipaddr
ATTRIBUTE	Altiga-Partitioning-Secondary-DHCP	129	ipaddr
ATTRIBUTE	Altiga-Partitioning-Premise-Rout	131	ipaddr
ATTRIBUTE	Altiga-Partitioning-Partition-Max-Sessions 132	string
ATTRIBUTE	Altiga-Partitioning-Mobile-IP-Key	133	string
ATTRIBUTE	Altiga-Partitioning-Mobile-IP-Address	134	ipaddr
ATTRIBUTE	Altiga-Partitioning-Mobile-IP-SPI	135	ipaddr
ATTRIBUTE	Altiga-Partitioning-Strip-Realm		136	integer
ATTRIBUTE	Altiga-Partitioning-Group		137	integer
ATTRIBUTE	Altiga-Group-Name			250	string

#  Altiga value
VALUE	Altiga-Allow-Alpha-Only-Passwords-G Allow		1
VALUE	Altiga-Allow-Alpha-Only-Passwords-G Disallow		0

VALUE Altiga-SEP-Card-Assignment-G/U         SEP1            1
VALUE Altiga-SEP-Card-Assignment-G/U         SEP2            2
VALUE Altiga-SEP-Card-Assignment-G/U         SEP3            4
VALUE Altiga-SEP-Card-Assignment-G/U         SEP4            8
VALUE Altiga-SEP-Card-Assignment-G/U         Any-SEP         15

VALUE Altiga-Priority-on-SEP-G/U             High            1
VALUE Altiga-Priority-on-SEP-G/U             Med-High        2
VALUE Altiga-Priority-on-SEP-G/U             Medium          3
VALUE Altiga-Priority-on-SEP-G/U             Med-Low         4
VALUE Altiga-Priority-on-SEP-G/U             Low             5

VALUE Altiga-Tunneling-Protocols-G/U         PPTP            1
VALUE Altiga-Tunneling-Protocols-G/U         L2TP            2
VALUE Altiga-Tunneling-Protocols-G/U         IPSec           4
VALUE Altiga-Tunneling-Protocols-G/U         L2TP/IPSec      8
VALUE Altiga-Tunneling-Protocols-G/U         PPTP-and-IPSec  5
VALUE Altiga-Tunneling-Protocols-G/U         All             15

VALUE	Altiga-IPSec-Authentication-G	None			0
VALUE	Altiga-IPSec-Authentication-G	RADIUS			1
VALUE	Altiga-IPSec-Authentication-G	LDAP			2
VALUE	Altiga-IPSec-Authentication-G	NTDomain		3
VALUE	Altiga-IPSec-Authentication-G	SDI			4
VALUE	Altiga-IPSec-Authentication-G	Internal		5

VALUE Altiga-IPSec-Allow-Passwd-Store-G/U    Allow           1
VALUE Altiga-IPSec-Allow-Passwd-Store-G/U    Disallow        0

VALUE Altiga-Use-Client-Address-G/U          Allow           1
VALUE Altiga-Use-Client-Address-G/U          Disallow        0

VALUE Altiga-PPTP-Min-Authentication-G/U     PAP             1
VALUE Altiga-PPTP-Min-Authentication-G/U     CHAP            2
VALUE Altiga-PPTP-Min-Authentication-G/U     EAP-MD5         4
VALUE Altiga-PPTP-Min-Authentication-G/U     EAP-GTC         8
VALUE Altiga-PPTP-Min-Authentication-G/U     EAP-TLS         16
VALUE Altiga-PPTP-Min-Authentication-G/U     MSCHAPv1        32
VALUE Altiga-PPTP-Min-Authentication-G/U     MSCHAPv2        64
VALUE Altiga-PPTP-Min-Authentication-G/U     Default         102

VALUE Altiga-L2TP-Min-Authentication-G/U     PAP             1
VALUE Altiga-L2TP-Min-Authentication-G/U     CHAP            2
VALUE Altiga-L2TP-Min-Authentication-G/U     EAP-MD5         4
VALUE Altiga-L2TP-Min-Authentication-G/U     EAP-GTC         8
VALUE Altiga-L2TP-Min-Authentication-G/U     EAP-TLS         16
VALUE Altiga-L2TP-Min-Authentication-G/U     MSCHAPv1        32
VALUE Altiga-L2TP-Min-Authentication-G/U     MSCHAPv2        64
VALUE Altiga-L2TP-Min-Authentication-G/U     Default         102

VALUE	Altiga-PPTP-Encryption-G	PPTP-40bit		2
VALUE	Altiga-PPTP-Encryption-G	PPTP-40-Encryption-Req	3
VALUE	Altiga-PPTP-Encryption-G	PPTP-128		4
VALUE	Altiga-PPTP-Encryption-G	PPTP-128-Encryption-Req	5
VALUE	Altiga-PPTP-Encryption-G	PPTP-40-or-128		6
VALUE	Altiga-PPTP-Encryption-G	PPTP-40-or-128-Encry-Req 7
VALUE	Altiga-PPTP-Encryption-G	PPTP-40-Stateless-Req	10
VALUE	Altiga-PPTP-Encryption-G	PPTP-40-Enc/Stateless-Req 11
VALUE	Altiga-PPTP-Encryption-G	PPTP-128-Stateless-Req	12
VALUE	Altiga-PPTP-Encryption-G	PPTP-128-Enc/Stateless-Req 13
VALUE	Altiga-PPTP-Encryption-G	PPTP-40/128-Stateless-Req 14
VALUE	Altiga-PPTP-Encryption-G	PPTP-40/128-Enc/Statls-Req 15

VALUE	Altiga-L2TP-Encryption-G	L2TP-40bit		2
VALUE	Altiga-L2TP-Encryption-G	L2TP-40-Encryption-Req	3
VALUE	Altiga-L2TP-Encryption-G	L2TP-128		4
VALUE	Altiga-L2TP-Encryption-G	L2TP-128-Encryption-Req	5
VALUE	Altiga-L2TP-Encryption-G	L2TP-40-or-128		6
VALUE	Altiga-L2TP-Encryption-G	L2TP-40-or-128-Encry-Req 7
VALUE	Altiga-L2TP-Encryption-G	L2TP-40-Stateless-Req	10
VALUE	Altiga-L2TP-Encryption-G	L2TP-40-Enc/Stateless-Req 11
VALUE	Altiga-L2TP-Encryption-G	L2TP-128-Stateless-Req	12
VALUE	Altiga-L2TP-Encryption-G	L2TP-128-Enc/Stateless-Req 13
VALUE	Altiga-L2TP-Encryption-G	L2TP-40/128-Stateless-Req 14
VALUE	Altiga-L2TP-Encryption-G	L2TP-40/128-Enc/Statls-Req 15

VALUE	Altiga-Argument-Authentication-Server-Type FirstActiveServer 1
VALUE	Altiga-Argument-Authentication-Server-Type RADIUS	1
VALUE	Altiga-Argument-Authentication-Server-Type LDAP		2
VALUE	Altiga-Argument-Authentication-Server-Type NT		3
VALUE	Altiga-Argument-Authentication-Server-Type SDI		4
VALUE	Altiga-Argument-Authentication-Server-Type Internal	5

VALUE	Altiga-IPSec-L2L-Keepalives-G	ON			1
VALUE	Altiga-IPSec-L2L-Keepalives-G	OFF			0

VALUE	Altiga-IPSec-Tunnel-Type-G	LAN-to-LAN		1
VALUE	Altiga-IPSec-Tunnel-Type-G	Remote-Access		2

VALUE	Altiga-IPSec-Mode-Config-G	ON			1
VALUE	Altiga-IPSec-Mode-Config-G	OFF			0

VALUE	Altiga-IPSec-User-Group-Lock-G	ON			1
VALUE	Altiga-IPSec-User-Group-Lock-G	OFF			0

VALUE	Altiga-IPSec-Over-NAT-G		ON			1
VALUE	Altiga-IPSec-Over-NAT-G		OFF			0

VALUE	Altiga-Partitioning-Strip-Realm	ON			1
VALUE	Altiga-Partitioning-Strip-Realm	OFF			0

END-VENDOR Altiga
